Planning Application – 2014/01163/FUL

Rear of Heritage Coast Visitor Centre, Dunraven Bay, Bridgend

Materials

1. Timber Cladding

Timber Cladding (dark stain) will be added to the visible elevations. Metal walls will be dark grey.

Side elevations

Timber cladding to be added to any overhang that is visible on the side elevation furthest from the visitor centre and the elevation facing the visitor’s centre.

The type of timber will be investigated to ensure that it is durable to withstand weather conditions and will not compromise the metal material.

Front Elevation

Timber cladding to be added to the front elevation.

Once the timber cladding has been identified it will require approval from the Local Planning Authority.

1. Roof

Roof will be dark grey/ matt black.

Sample of colour to be provided for agreement by the Local Planning Authority.

1. Roller Shutter Doors

Roller shutter doors to be dark grey.

Sample of colour to be provided for agreement by the Local Planning Authority.